Cody Mitchell
Structural and Pipe Welder
Tulsa, OK  |  cody.mitchell@example.com  |  (918) 555-0141
SUMMARY
AWS Certified Welder with 7 years of experience in structural steel fabrication and process piping, certified in SMAW and FCAW to AWS D1.1 in all plate positions and qualified on 6G pipe. Keeps a weld repair rate under 1% on welds checked by ultrasonic and visual inspection. Reads shop drawings and welding symbols, sets up from the WPS and runs plasma, track torch and oxy-fuel cutting equipment.
EXPERIENCE
Structural Welder	Mar 2021 - Present
Northwind Steel Fabricators, Tulsa, OK
Weld beams, columns, moment connections and base plates for commercial buildings using FCAW and SMAW to AWS D1.1, averaging 40+ linear feet of fillet and groove welds per shift.
Keep a weld repair rate under 1% on welds checked by third-party ultrasonic testing (UT) and visual inspection across 3 years of projects.
Read shop drawings and AWS welding symbols to fit up assemblies within 1/16 inch before welding.
Cut and bevel plate and pipe with plasma, track torch and oxy-fuel equipment, cutting fit-up rework on the crew by about a third.
Trained 4 apprentice welders on machine setup, preheat checks and interpass cleaning, and all 4 passed their D1.1 bend tests on the first attempt.
Follow hot work permits, fire watch and PPE rules, with zero lost-time incidents in 4 years.
Welder	Jun 2018 - Feb 2021
Contoso Industrial Services, Broken Arrow, OK
Welded carbon steel process piping from 2 to 12 inches using GTAW root passes with SMAW fill and cap, in the shop and at plant shutdowns.
Passed radiographic testing (RT) on 48 of 48 sampled production pipe welds during a 6-week refinery turnaround.
Fit and tacked pipe spools with stands, clamps and 2-hole pins to match isometric drawings.
Maintained welding machines, leads and grinders and logged rod oven temperatures each shift to keep low-hydrogen electrodes in storage requirements.
EDUCATION
Welding Technology Certificate, Arrowhead Technical College, Tulsa, OK	2018
LICENSES AND CERTIFICATIONS
AWS Certified Welder, AWS D1.1 Structural Steel, SMAW 3G and 4G plate, unlimited thickness, American Welding Society
AWS Certified Welder, AWS D1.1 Structural Steel, FCAW 3G and 4G plate, unlimited thickness, American Welding Society
Welder performance qualification, ASME Section IX, 6G carbon steel pipe, GTAW root with SMAW fill and cap
OSHA 10-Hour Construction, OSHA Outreach Training Program
SKILLS
SMAW (stick)  •  FCAW (flux core)  •  GTAW (TIG)  •  GMAW (MIG)  •  AWS D1.1 structural welding  •  6G pipe welding  •  Blueprint and welding symbol reading  •  Fit-up and tacking  •  Plasma, track torch and oxy-fuel cutting  •  Visual weld inspection  •  Hot work safety




